****

**September 2019**

**2015/863/EU (RoHS 3 Directive)**

**PCB’s Supplied by Hi Spec Corporation Limited.**

All Printed Circuit Boards supplied with the following Surface Finishes:-

**Electroless Nickel / Immersion Gold**

**Immersion Tin**

**Immersion Silver**

**Electroplated Gold**

**Electroless Nickel / Electroless Palladium/ Immersion Gold**

**Lead Free Hot Air Levelling**

Will conform to the Directive (EU) 2015/863 amendment of the RoHS 3 DIRECTIVE

2011/65/EU, RoHS-Recast, Article 4(1): and do not contain any of the below mentioned

10 Hazardous substances.

** Cadmium (Cd)**

** Mercury**

** Lead (Pb)**

** Hexavalent chromium (Cr6+)**

** Polybrominated biphenyls (PBB)**

** Polybrominated diphenyl ethers (PBDE)**

** Bis(2-Ethylhexyl) phthalate (DEHP) (added in 2015)**

** Benzyl butyl phthalate (BBP) (added in 2015)**

** Dibutyl phthalate (DBP) (added in 2015)**

** Diisobutyl phthalate (DIBP) (added in 2015)**

**If you would like any additional information on “RoHS 3” please contact Robert Allan on +44 (0) 1489 889966 or email** [**sales@hispecltd.co.uk**](mailto:sales@hispecltd.co.uk)

**Best regards**

**R Allan**

**Robert Allan**

**Director**